======================================================================== 
Keelung/ShinYi FW 362 change list 
                   
Date: 20141106

1. Fixes an USB enumeration porblem while keyboard is plugged in 5V USB port of 4900-7x5 system unit
2. Fixes an issue where W303 error logged on 4690 OS

======================================================================== 
Yami FW 0412 change list 
                   
Date: 20141204
======================================================================== 

To change in the FW0412 base on Keelung V0362 should be as below:

1. XB293024 -The standard 5V USB would drop down to low voltage while warm boot the Jade system
2. XB295772 - W303 error logged on 4690 because LED cmd did not respond correctly
   XB296614 - Cmd reject response from 4820 fw 0411
